To: **Estimating Department**

# Bid Proposal

This Proposal supersedes, cancels and withdraws all previous submissions

## References:

NFPA 13: Installation of Sprinkler Systems.

NFPA 72: National Fire Alarm Code.

NFPA 170: Standard for Fire Safety and Emergency Symbols.

Incorporated into this document are other NFPA Codes as referenced and where applicable.

Ref: <http://www.nfpa.org/aboutthecodes/list_of_codes_and_standards.asp>

EN 12845: Fixed firefighting systems, Automatic sprinkler systems, Design, installation and maintenance where applicable.

International Fire & Building Code/s and Life Safety Code.

## Summary

This proposal is to supply Parts & Smarts for an automatic fire alarm system for JOB SITE NAME AND ADDRESS, all levels, in accordance with the above referenced standards where applicable, and in accordance with approved Drawings, Calculations and Permits, and all addendums as released as of 2016-mm-dd

## Inclusions

1. The supply of:
   1. All Parts & materials for the Fire Alarm System and Panel including:
      1. One (1) Edwards-Mirtone VS-1 Fire Panel (FACP)
      2. Edwards Voice Evacuation Control Panel (1)
      3. Speaker/Horn strobes, (38 speaker/horn/strobe + 15 strobe only)
      4. Weatherproof Horn/Strobe (1) (Faces the street warning no entry)
      5. Smoke detectors, (4) Sounder bases, (0)
      6. Pull stations near exits, (1)
      7. Fire alarm modules. (4)
      8. Control relays for elevator recalls (4)
      9. Booster Power Supplies (1)
      10. Class-A NAC adapter/s (1)
   2. Programming of Edward VS-1 Fire Alarm Panel (1)
2. Proofing:
   1. Inspecting the System,
   2. Test the System which includes
      1. Final fire inspection with AHJ (1)
      2. Supply final fire inspection report to FSS PM & General. (1).

## Exclusions

1. Design, Submittals & Permit
2. Installation of Fire Alarms System LV & HV supply and wiring runs.
3. Fire Suppression Sprinkler System Installation. . (A separate Proposal IS/IS NOT attached)
4. Portable Fire Extinguishers. (A separate Proposal IS/IS NOT attached)
5. All underground piping installation. (A separate Proposal IS/IS NOT attached)

## Additional Charges

* Remote Monitoring Services. Can be supplied by **Fire Suppression Services Inc.**
* Any extra programming of the FACP. (i.e. if additional devices are added via Change Order or AHJ.)

## Notes to Owner/Architect

**Parts & Smarts means:** We are providing the Electrical Contractor with the Devices. They do the installation.

If we advise on the installation extra charges will be billed to you..

It is Owner’s responsibility to supply 120 VAC 15-20 Amp, dedicated circuit with dedicated ground wiring and connectivity to building fire alarm panels and electrical breakers. **Fire Suppression Services Inc.** technicians are not High Voltage AC electricians.

Responsibility in Electrical Contractor’s Scope of work should be:

1. Power supply and wiring work pertaining to the Fire Alarm System for

1.1. Wiring alarm bell/gong (external over the FDC)

1.2. Wiring alarm and trip devices.

1.3. Wiring low Voltage Electrical work to connect …:

1.3.1. Alarms,

1.3.2. Strobes,

1.3.3. Bells,

1.3.4. Flow & tamper devices

.. Back to building fire alarm panels.

Owner to advise FSS on the choice of dialer - wired or wireless.

**Electrical Contractor:** If Owner chooses not to use wireless dialer, then you must run Cat-6 phone lines from De-Marc to Fire Panel. YOU must supply dialtone before finals (no voicemail. The ‘stutter’ interferes with line-seizure). (We will do the termination at the panel)

Owner will be required to have off-site monitoring by a remote service, of all alarms. (Code)

NOTE: **Fire Suppression Services Inc.** can supply this service on request at an additional annual rate charge.

Owner to advise alarm technicians when sprinkler division has completed riser main and main & subsidiary FDC tamper switches are installed.

# Addenda

**These addenda are our TERMS & CONDITIONS and are incorporated into the Proposal in its entirety.**

## BILLING & PAYMENT

## All our Requests for Payment (billing) will be submitted per AIA docs “G702 Application for Progress Payment” using the AIA G703 “Continuation Sheet” “Schedule of Values”. The Progress Payment you make is part of an Invoice that represents the full amount of the Contract. We use ONE Master Invoice number for the project. Your payments are progress payments against this invoice. IF we issue YOU this Invoice, then: ALL invoice amounts (the full Contract Amount), on this invoice are Net 15, no exception. FSS will register the job with the Utah State Construction Service and will at all times preserve its lien rights. Property Owner will be notified and a lien placed on the property if amounts due are unpaid after 30 days from the application for payment date.

## BOND (ADDITIONAL CHARGE)

If requested, Fire Suppression Services Inc. shall furnish Bonds in the form requested by you, the 'Owner', covering the faithful performance of the Agreement, and the payment of all obligations arising there under. These may be in the form of 100% Performance, 100% Labor and Material Payment, and Lien Bonds.

The FULL cost of providing such Bond/s for you, the Owner and/or his Agent/Contractor shall be paid by you, the Owner/Agent/Contractor or whosoever may require Fire Suppression Services Inc. to furnish said Bond/s, and is an additional cost/amount, and IS NOT included in this bid.

Any and all payments required by Fire Suppression Services Inc. for the above shall be shown on any Breakout Sheet (e.g.: AIA-G703) as a SEPARATE item list and shall NOT be subject to any “retainage”.

This Subcontractor shall be reimbursed, without any retainage, for the cost of any required performance or payment bonds simultaneously with the FIRST progress payment.

## CHANGES, CCO & PCO

All fire sprinkler nozzles and/or pipe-work AND All Hood Systems and their Suppression devices

AND: All Chemical Suppression Systems AND Portable Extinguishers AND: All Alarm Systems, will be installed as per approved Plans; Any change or deviations from said Plans will not be done without approved Change Order/s with attendant cost adjustments.

## CONTRACT

Seller objects to modifications and additions to any of the terms of this document, irrespective of the wording of the Purchasers acceptance, or other Purchaser Forms, Purchasers Contract, other Documents or hand written annotations on this Document. This document in its entirety is to be incorporated into ‘The Contract’ with you.

## FREIGHT

All goods that attract freight are FOB Origin FC.

## LABOR

Labor is calculated at a regular day rate and will be performed during business hours. (08:00-16:30) or (07:00-15:30) Hours outside these, or weekends are additional charge to you at time and one half, without exception & must be approved via CO, before worked.

## MOBILIZATION-DEMOBILIZATION-REMOBILIZATION

If Fire Suppression Services Inc. or its subcontractors have to suspend work, for any reason, and have to demobilize before completion, then we are entitled to recover our demobilization costs from you; and, if Fire Suppression Services Inc. and/or its subcontractors have to remobilize we are entitled to recover the remobilization costs from you.

## PERMIT, DESIGNS and SUBMITTALS

Any and all payments required by Fire Suppression Service Inc. for Permit, Designs & Submittals shall be shown on any Breakout Sheet (e.g.: AIA-G703) as a SEPARATE item list and shall NOT be subject to any “retainage”.

## Prices & Taxes

If Seller is required to pay any taxes or other fees relating to the services to be performed or to the production, sale or transportation of goods, Purchaser will reimburse the Seller for any such taxes or fees. Portable Fire Extinguishers attract Utah Sales Tax.

## Attorneys Fees

In the event that either party brings an action or proceeding for a declaration of the rights of the parties under this Agreement, for injunctive relief, or for an alleged breach or default of this Agreement, or any other action arising out of or related to this Agreement or the transactions contemplated hereby, the prevailing party in any such action will be entitled to an award of reasonable attorneys’ fees, expenses and costs (including, without limitations, expert fees) incurred in such action or proceeding, in addition to any other damages or relief awarded, regardless of whether such action proceeds to final judgment.

**You agree to pay all outstanding Statement amounts, and all interest, attorney’s fees and collection costs**.

## Right of Way

Fire Suppression Services requires first right of way; this means that Fire Suppression Sprinkler Technician/Fitters “must be First & High”.

## Tamper

Tampering or Adjusting or Working on Fire Suppression installed and tagged Systems by anyone other than Fire Suppressions Authorized personnel or Certified /Authorized / Licensed Fire Protection Service Personnel not only jeopardizes the safe and correct operation of the equipment; it voids the tags on said System, voids all **FSS** Warrantees, and it is highly likely it will affect your Insurance.

Unless your maintenance department personnel are so authorized, it is advisable to leave the System equipment maintenance and servicing to Certified Personnel.

## Asbestos Notice:

**FIRE SUPPRESSION SERVICES Inc. IS NEITHER FORMALLY LICENSED IN THE REMOVAL OF, NOR THE ANALYSIS OF ASBESTOS.** OUR COMPANY WILL THEREFORE NOT NORMALLY DEAL WITH ALL ASBESTOS RELATED INCIDENTS IN A PRACTICAL SENSE ON BEHALF OF OUR CLIENTS. WHEN THE PRESENCE OF ASBESTOS IS SUSPECTED WE WILL STOP WORK AND APPOINT COMPETENT AND ACCREDITED SUB CONTRACTORS ON A SITE-SPECIFIC BASIS TO CARRY OUT ANY REMOVALS OR TEST

2016-08-19